{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","","","","41","46","47"]
["","","","Stredný","dBA","","","","38","42","43"]
["","","","Nízka","dBA","","","","35","39","40"]
["","Chladenie","","Stredný","dBA","","","","38","42","43"]
["","","","Nízka","dBA","","","","35","39","40"]
["","","","Vysoké","dBA","","","","41","46","47"]
["Štandardné príslušenstvo","Návod na prevádzku","","","","","","","1","1","1"]
["","Návod na montáž","","","","","","","1","1","1"]
["","Vypúšťacia hadica","","","","","","","1","1","1"]
["","Tepelná izolačná rúrka","","","","","","","3","3","3"]
["","Upínacie pásy","","","","","","","10","10","10"]
["","Pás hadice","","","","","","","1","1","1"]
["","Tesniaci materiál","","","","","","","4","4","4"]
["","Upevňovacia doska podložky","","","","","","","1","1","1"]
["","Vypúšťací spoj","","","","","","","1","1","1"]
["","Netkaná látka","","","","","","","1","1","1"]
["","Podložka","","","","","","","8","8","8"]
["","Upevňovacia skrutka pre odvodovú hadicu","","","","","","","5","5","5"]
["Riadiace systémy","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Chladiaci výkon","Celkový výkon","","Men.","kW","","","","","","12.1"]
["Pripojenia potrubí","Kvapalina","","OD","mm","","","","9.52","9.52","9.52"]
["","Plyn","","OD","mm","","","","15.9","15.9","15.9"]
["","Vypúšťanie","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Chladenie","","","dBA","","","","59","64","65"]
["","Vykurovanie","","","dBA","","","","59","64"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","","","","950","950","950"]
["","","","Hĺbka","mm","","","","950","950","950"]
["","","","Výška","mm","","","","198","198","198"]
["Opláštenie","Materiál","","","","","","","Živica","Živica","Živica"]
["","Farba","","","","","","","Jasná biela","Jasná biela","Jasná biela"]
["Hmotnosť","Jednotka","","","kg","","","","25.0","26.0","26"]
["Ventilátor","Prietok vzduchu","Kúrenie","Vysoké","m³/min","","","","23.0","31.0","32.5"]
["","","","Stredný","m³/min","","","","19.5","25.5","26.5"]
["","","","Nízka","m³/min","","","","16.0","20.0","20.5"]
["","","Chladenie","Nízka","m³/min","","","","16.0","20.0","20.5"]
["","","","Stredný","m³/min","","","","19.5","25.5","26.5"]
["","","","Vysoké","m³/min","","","","23.0","31.0","32.5"]
["Výška odsávania","mm","","","","","","","600","600","600"]
["Vykurovací výkon","Celkový výkon","","Nom. ot.","kW","","","","","","13.5"]
["Opláštenie","Farba","","","","Jasná biela","Jasná biela","Jasná biela"]
["","Materiál","","","","Živica","Živica","Živica"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","198","198","198"]
["","","","Šírka","mm","950","950","950"]
["","","","Hĺbka","mm","950","950","950"]
["Hmotnosť","Jednotka","","","kg","25.0","26.0","26.0"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","23.0","31.0","32.5"]
["","","","Stredný","m³/min","19.5","25.5","26.5"]
["","","","Nízka","m³/min","16.0","20.0","20.5"]
["","","Kúrenie","Vysoké","m³/min","23.0","31.0","32.5"]
["","","Vykurovanie","Stredný","m³/min","19.5","25.5","26.5"]
["","","Kúrenie","Nízka","m³/min","16.0","20.0","20.5"]
["Akustický výkon","Chladenie","","","dBA","59","64","65"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","41","46","47"]
["","","","Stredný","dBA","38","42","43"]
["","","","Nízka","dBA","35","39","40"]
["","Kúrenie","","Vysoké","dBA","41","46","47"]
["","Vykurovanie","","Stredný","dBA","38","42","43"]
["","Kúrenie","","Nízka","dBA","35","39","40"]
["Pripojenia potrubia","Kvapalina","","OD","mm","9.52","9.52","9.52"]
["","Plyn","","OD","mm","15.9","15.9","15.9"]
["","Odvod kondenzátu","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Výška odsávania","mm","","","","600","600","600"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Chladiaci výkon","Celkový výkon","","Men.","kW","","","12.10"]
["Vykurovací výkon","Celkový výkon","","Nom. ot.","kW","","","13.5"]