{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUQ100CVEB / RZQG71L8Y1B","FUQ71CVEB / RZQG71L8Y1B","FUQ71CVEB / FUQ71CVEB / RZQG100L8Y1B","FUQ71CVEB / FUQ71CVEB / RZQG125L8Y1B"]
["Chladiaci výkon","Men.","","kW","","6.8"]
["Space cooling","SEER","","","6.50","6.42","5.10","5.10"]
["","Ročná spotreba energie","","kWh/a","367","371","652","824"]
["","Výkon","P návrh","kW","6.80","6.80","9.50","12.00"]
["","Trieda energetickej účinnosti","","","A++","A++","B","B"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","7.60","7.60","11.30","12.71"]
["","SCOP/A","","","4.20","4.20","3.80","3.80"]
["","Trieda energetickej účinnosti","","","A+","A+","A","A"]
["","Ročná spotreba energie","","kWh/a","2,534","2,534","4,164","4,683"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","","840"]
["","EER","","","","4.05"]
["","COP","","","","4.08"]
["","Smernica o energetickom označovaní","Chladenie","","","A"]
["","","Vykurovanie","","","A"]
["Vykurovací výkon","Men.","","kW","","7.5"]
["Poznámky","","","","","(1) - Ročná spotreba energie je podľa Smernice o energetickom označení 2002/31/ES"]
["","","","","","(2) - Hodnoty SEER a SCOP sú podľa normy EN 14825"]