{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":9,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A"]
[]
[]
[]
[]
["","","","","","FVA140AMVEB","FVA71AMVEB","FVA100AMVEB","FVA125AMVEB"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","53"]
["","","","Men.","dBA","51"]
["","","","Stredný","dBA","48"]
["","Chladenie","","Stredný","dBA","51"]
["","","","Nízka","dBA","48"]
["","","","Vysoké","dBA","53"]
["Štandardné príslušenstvo","Skrutky","","","","5"]
["","Návod na montáž","","","","1"]
["","Návod na prevádzku","","","","1"]
["","Puzdro","","","","1"]
["","Upínacie pásy","","","","5"]
["","Izolácia príslušenstva pre plynové potrubie","","","","1"]
["","Izolácia príslušenstva pre potrubie s kvapalinou","","","","1"]
["","Materiál odolný voči roseniu","","","","1"]
["","Káble diaľkového ovládača","","","","1"]
["","Konzola na inštaláciu","","","","1"]
["","Ochranná gumená priechodka","","","","2"]
["","Kryt","","","","1"]
["","Inštalačná šablóna","","","","1"]
["Riadiace systémy","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Chladiaci výkon","Celkový výkon","","Men.","kW","13.40"]
["Pripojenia potrubí","Kvapalina","","OD","mm","9.52"]
["","Plyn","","OD","mm","15.9"]
["","Vypúšťanie","","","","I.D. 20/O.D. 26"]
["Sound power level","Chladenie","","","dBA","65"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","600"]
["","","","Hĺbka","mm","350"]
["","","","Výška","mm","1,850"]
["Opláštenie","Farba","","","","Jasná biela"]
["Hmotnosť","Jednotka","","","kg","50"]
["Ventilátor","Prietok vzduchu","Kúrenie","Vysoké","m³/min","30"]
["","","","Stredný","m³/min","28"]
["","","","Nízka","m³/min","26"]
["","","Chladenie","Nízka","m³/min","26"]
["","","","Stredný","m³/min","28"]
["","","","Vysoké","m³/min","30"]
["Vykurovací výkon","Celkový výkon","","Nom. ot.","kW","15.5"]
["Power supply","Fáza","","","","1~"]
["","Frekvencia","","","Hz","50/60"]
["","Napätie","","","V","220-240/220"]
["Poznámky","","","","","(1) - Elektrické údaje nájdete v samostatných nákresoch","","(1) - Elektrické údaje nájdete v samostatných nákresoch"]
["Opláštenie","Farba","","","","","Jasná biela","Jasná biela","Jasná biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","1850","1850","1850"]
["","","","Šírka","mm","","600","600","600"]
["","","","Hĺbka","mm","","270","350","350"]
["Hmotnosť","Jednotka","","","kg","","42","50","50"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","","18","28","28"]
["","","","Stredný","m³/min","","16","25","26"]
["","","","Nízka","m³/min","","14","22","24"]
["","","Kúrenie","Vysoké","m³/min","","18","28","28"]
["","","Vykurovanie","Stredný","m³/min","","16","25","26"]
["","","Kúrenie","Nízka","m³/min","","14","22","24"]
["Akustický výkon","Chladenie","","","dBA","","55","62","63"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","","43","50","51"]
["","","","Stredný","dBA","","41","47","48"]
["","","","Nízka","dBA","","38","44","46"]
["","Kúrenie","","Vysoké","dBA","","43","50","51"]
["","Vykurovanie","","Stredný","dBA","","38","44","46"]
["","Kúrenie","","Men.","dBA","","41","47","48"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","9.52","9.52","9.52"]
["","Plyn","","OD","mm","","15.9","15.9","15.9"]
["","Odvod kondenzátu","","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Riadiace systémy","Káblový diaľkový ovládač","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Štandardné príslušenstvo","Installation manual","","","","","1","1","1"]
["","Hole protection rubber","","","","","2","2","2"]
["","Cover","","","","","1","1","1"]
["","Dew proof material","","","","","1","1","1"]
["","Remote control wiring","","","","","1","1","1"]
["","Bracket for installation","","","","","1","1","1"]
["","Operation manual","","","","","1","1","1"]
["","Bush","","","","","1","1","1"]
["","Installation pattern","","","","","1","1","1"]
["","Insulation for fitting for gas pipe","","","","","1","1","1"]
["","Insulation for fitting for liquid pipe","","","","","1","1","1"]
["","Screws","","","","","5","5","5"]
["","Tie-wraps","","","","","5","5","5"]
["Napájanie","Fáza","","","","","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","50/60","50/60","50/60"]
["","Napätie","","","V","","220-240/220","220-240/220","220-240/220"]
["Chladiaci výkon","Celkový výkon","","Men.","kW","","","","12.10"]
["Vykurovací výkon","Celkový výkon","","Nom. ot.","kW","","","","13.5"]