{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Hladina akust. tlaku","Kúrenie","Vysoké","dBA","43","50","51","53"]
["","","Men.","dBA","41","47","48","51"]
["","","Nízka","dBA","38","44","46","48"]
["","Chladenie","Nízka","dBA","38","44","46","48"]
["","","Vysoké","dBA","43","50","51","53"]
["","","Men.","dBA","41","47","48","51"]
["Štandardné príslušenstvo","Návod na prevádzku","","","Návod na prevádzku","Návod na prevádzku","Návod na prevádzku","Návod na prevádzku"]
["","Návod na montáž","","","Návod na montáž","Návod na montáž","Návod na montáž","Návod na montáž"]
["","Konzola na inštaláciu","","","Konzola na inštaláciu","Konzola na inštaláciu","Konzola na inštaláciu","Konzola na inštaláciu"]
["","Ochranná gumená priechodka","","","Ochranná gumená priechodka","Ochranná gumená priechodka","Ochranná gumená priechodka","Ochranná gumená priechodka"]
["","Puzdro","","","Puzdro","Puzdro","Puzdro","Puzdro"]
["","Izolácia príslušenstva","","","Izolácia príslušenstva","Izolácia príslušenstva","Izolácia príslušenstva","Izolácia príslušenstva"]
["","Kryt","","","Kryt","Kryt","Kryt","Kryt"]
["","Svorky","","","Svorky","Svorky","Svorky","Svorky"]
["","Skrutky","","","Skrutky","Skrutky","Skrutky","Skrutky"]
["","Inštalačná šablóna","","","Inštalačná šablóna","Inštalačná šablóna","Inštalačná šablóna","Inštalačná šablóna"]
["","Materiál odolný voči roseniu","","","Materiál odolný voči roseniu","Materiál odolný voči roseniu","Materiál odolný voči roseniu","Materiál odolný voči roseniu"]
["","Káble diaľkového ovládača","","","Káble diaľkového ovládača","Káble diaľkového ovládača","Káble diaľkového ovládača","Káble diaľkového ovládača"]
["Riadiace systémy","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Pripojenia potrubia","Kvapalina","OD","mm","9.52","9.52","9.52","9.52"]
["","Plyn","OD","mm","15.9","15.9","15.9","15.9"]
["","Vypúšťanie","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Vstup napájania","Chladenie","Men.","kW","0.117","0.238","0.238","0.276"]
["","Kúrenie","Men.","kW","0.117","0.238","0.238","0.276"]
["Úroveň akustického výkonu","Chladenie","","dBA","55","62","63","65"]
["","Vykurovanie","","dBA","55","62","63","65"]
["Vonkajšie rozmery","Jednotka","Šírka","mm","600","600","600","600"]
["","","Hĺbka","mm","270","350","350","350"]
["","","Výška","mm","1,850","1,850","1,850","1,850"]
["Kryt","Farba","","","Jasná biela","Jasná biela","Jasná biela","Jasná biela"]
["Hmotnosť","Jednotka","","kg","39","47","47","47"]
["Power supply","Fáza","","","1~","1~","1~","1~"]
["","Frekvencia","","Hz","50/60","50/60","50/60","50/60"]
["","Napätie","","V","220-240/220","220-240/220","220-240/220","220-240/220"]