{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXLG-M"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXLG25M2V1B","FVXG35K2V1B / RXLG35M2V1B"]
["Outdoor unit","","","","RXLG25M","RXLG35M"]
["Chladiaci výkon","Min.","","kW","1.2","1.4"]
["","Men.","","kW","2.5","3.5"]
["","Max.","","kW","5.1","5.6"]
["Vykurovací výkon","Min.","","kW","1.0","1.1"]
["","Men.","","kW","4.5","5.6"]
["","Max.","","kW","6.5, 3.5","7.0, 4.0"]
["Nominálna účinnosť","EER","","","3.52","3.43"]
["","COP","","","3.88","3.61"]
["","Ročná spotreba energie","","kWh","355","510"]
["","Smernica o energetickom označovaní","Chladenie","","A","A"]
["","","Vykurovanie","","A","A"]
["Pripojenia potrubí","Vypúšťanie","OD","mm","18","18"]
["Pripojenia potrubia","Plyn","OD","mm","9.5","9.5"]
["","Kvapalina","OD","mm","6.35","6.35"]
["Chladenie","Trieda energetickej účinnosti","","","A++","A++"]
["","Výkon","P návrh","kW","2.50","3.50"]
["","SEER","","","6.99","6.59"]
["","Ročná spotreba energie","","kWh/a","131","186"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","A+","A+"]
["","Výkon","P návrh","kW","3.00","3.40"]
["","SCOP/A","","","4.25","4.01"]
["","Ročná spotreba energie","","kWh/a","988","1187"]
["Poznámky","","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]
["","","","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]
["","","","","(3) - 220 V","(3) - 220 V"]
["","","","","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240 V","(5) - 240 V"]
["","","","","(6) - Pre nominálny minimálny vykurovací výkon je ventilátor vnútornej jednotky nastavený na SL","(6) - Pre nominálny minimálny vykurovací výkon je ventilátor vnútornej jednotky nastavený na SL"]
["","","","","(7) - Maximálny vykurovací výkon pri vonkajšej teplote -15°C","(7) - Maximálny vykurovací výkon pri vonkajšej teplote -15°C"]