{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":8,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B"]
[]
[]
[]
[]
["","","","","","FVXM25B2V1B","FVXM35B2V1B","FVXM50B2V1B"]
["Vstup napájania","Chladenie","","Men.","kW","0.02","0.02","0.03"]
["","Kúrenie","","Men.","kW","0.02","0.03","0.03"]
["Opláštenie","Farba","","","","Biela","Biela","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","600","600","600"]
["","","","Šírka","mm","750","750","750"]
["","","","Hĺbka","mm","238","238","238"]
["Hmotnosť","Jednotka","","","kg","17","17","17"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","8.7","9.2","11.6"]
["","","","Stredný","m³/min","7","7","9"]
["","","","Nízka","m³/min","4.9","4.9","6.6"]
["","","","Tichá prevádzka","m³/min","4.1","4.1","5.4"]
["","","Kúrenie","Vysoké","m³/min","9.2","9.8","12.8"]
["","","Vykurovanie","Stredný","m³/min","7.2","7.2","10"]
["","","Kúrenie","Nízka","m³/min","5.6","5.6","8.4"]
["","","","Tichá prevádzka","m³/min","4.1","4.1","5.9"]
["Akustický výkon","Chladenie","","","dBA","52","53","61"]
["","Vykurovanie","","","dBA","52","53","62"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","38","39","44"]
["","","","Stredný","dBA","32","32","38"]
["","","","Nízka","dBA","25","25","31"]
["","","","Tichá prevádzka","dBA","20","20","27"]
["","Kúrenie","","Vysoké","dBA","38","39","46"]
["","Vykurovanie","","Stredný","dBA","32","32","40"]
["","Kúrenie","","Nízka","dBA","25","25","35"]
["","","","Tichá prevádzka","dBA","19","19","29"]
["Chladivo","GWP","","","","675","675","675"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.4","6.4","6.4"]
["","Plyn","","OD","mm","9.5","9.5","12.7"]
["","Odvod kondenzátu","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","ARC466A90","ARC466A90","ARC466A90"]
["","Káblový diaľkový ovládač","","","","BRC073A1","BRC073A1","BRC073A1"]
["Štandardné príslušenstvo","FVXM25B2V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Napájanie","Názov","","","","V1","V1","V1"]
["","Fáza","","","","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35°CDB, 24°CWB; ekvivalentná dĺžka potrubia: 5m","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35°CDB, 24°CWB; ekvivalentná dĺžka potrubia: 5m","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35°CDB, 24°CWB; ekvivalentná dĺžka potrubia: 5m"]
["","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m"]
["Štandardné príslušenstvo","FVXM35B2V1B","","","","","1"]
["","FVXM50B2V1B","","","","","","1"]