{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-B"]
[]
[]
[]
[]
["","","","","","FVXTM30B2V1B"]
["Vstup napájania","Chladenie","","Men.","kW","0.02"]
["","Kúrenie","","Men.","kW","0.03"]
["Opláštenie","Farba","","","","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","600"]
["","","","Šírka","mm","750"]
["","","","Hĺbka","mm","238"]
["Hmotnosť","Jednotka","","","kg","17"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","9"]
["","","","Stredný","m³/min","6.7"]
["","","","Nízka","m³/min","4.8"]
["","","","Tichá prevádzka","m³/min","4"]
["","","Kúrenie","Vysoké","m³/min","9.4"]
["","","Vykurovanie","Stredný","m³/min","6.8"]
["","","Kúrenie","Nízka","m³/min","5.3"]
["","","","Tichá prevádzka","m³/min","4"]
["Akustický výkon","Chladenie","","","dBA","53"]
["","Vykurovanie","","","dBA","53"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","39"]
["","","","Stredný","dBA","32"]
["","","","Nízka","dBA","25"]
["","","","Tichá prevádzka","dBA","20"]
["","Kúrenie","","Vysoké","dBA","39"]
["","Vykurovanie","","Stredný","dBA","32"]
["","Kúrenie","","Nízka","dBA","25"]
["","","","Tichá prevádzka","dBA","19"]
["Chladivo","GWP","","","","675"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35"]
["","Plyn","","OD","mm","9.5"]
["","Odvod kondenzátu","","","","VP20 (I.D. 20/O.D. 26)"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","ARC466A90"]
["","Káblový diaľkový ovládač","","","","BRC073A1"]
["Štandardné príslušenstvo","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Napájanie","Názov","","","","V1"]
["","Fáza","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50"]
["","Napätie","","","V","220-240"]
["Poznámky","","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35°CDB, 24°CWB; ekvivalentná dĺžka potrubia: 5m"]
["","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m"]
["","","","","","(3) - Elektrické údaje nájdete v samostatných nákresoch"]