{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Štandardné príslušenstvo","Návod na montáž","","","","1"]
["","Návod na prevádzku","","","","1"]
["","Pripájanie potrubia","","","","1"]
["","Štítok chladiacej látky pre reguláciu plynu F","","","","1"]
["","Štítok s náplňou chladiva","","","","1"]
["","Viacjazyčné štítky o fluórovaných skleníkových plynoch","","","","1"]
["Hmotnosť","Jednotka","","","kg","370"]
["Chladiace médium","Charge","","","TCO2Eq","24.0"]
["","GWP","","","","2,087.5"]
["","Náplň","","","kg","11.5"]
["","Typ","","","","R-410A"]
["Motor ventilátora","Výkon","","","W","750"]
["","Pohon","","","","Priamy pohon"]
["Výmenník tepla","Typ","","","","Špirála priečnych lamiel"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","1,240"]
["","","","Hĺbka","mm","765"]
["","","","Výška","mm","1,680"]
["Opláštenie","Colour","","","","Slonovinovo biela"]
["Ventilátor","Type","","","","Axiálny ventilátor"]
["","Prietok vzduchu","Chladenie","Men.","m³/min","230"]
["","Množ.","","","","2"]
["Power supply","Fáza","","","","3~"]
["","Frekvencia","","","Hz","50"]
["","Voltage","","","V","380-415"]
["Poznámky","","","","","(1) - Režim priority chladenia: vnútorná teplota: 27°CDB, 19°CWB; vonkajšia teplota 32°CDB; dĺžka potrubia: 7,5 m; úroveň hladiny: 0 m"]
["","","","","","(2) - Režim priority chladenia: odparovacia teplota -10℃; vonkajšia teplota 32°CDB; Sanie SH: 10℃"]
["","","","","","(3) - Režim 100 % rekuperácie tepla: vnútorná teplota: 20°CDB; vonkajšia teplota 7°CDB, 6°CWB; chladenie pri zaťažení 18 kW; dĺžka potrubia: 7,5 m; úroveň hladiny: 0 m"]
["","","","","","(4) - Nasýtená teplota ekvivalentná nasávaciemu tlaku (strana chladenia): -10 °C (pri chladenom stave); výkon spojenia pre vnútornú klimatizáciu: 10 HP, keď je rekuperácia tepla 100 %"]
["","","","","","(5) - Kompresor 1"]
["","","","","","(6) - Kompresor 2"]
["","","","","","(7) - Kompresor 3"]
["","","","","","(8) - Náplň jednotky z výroby"]
["","","","","","(9) - Namontujte lapač oleja na 5 m od vonkajšej jednotky"]
["","","","","","(10) - Viac podrobností nájdete na nákrese prevádzkového rozsahu"]
["","","","","","(11) - Podrobnosti o štandardnom príslušenstve nájdete v návode na montáž/prevádzku"]
["","","","","","(12) - Obsahuje fluórované skleníkové plyny"]