{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Typ","","","","","Čistič vzduchu"]
["Použitie","","","","","Parapetný typ"]
["Casing","Colour","","","","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","500"]
["","","","Šírka","mm","270"]
["","","","Hĺbka","mm","270"]
["Hmotnosť","Jednotka","","","kg","6.8"]
["Použiteľná oblasť v miestnosti","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Prevádzka čističky vzduchu","Vstup napájania","","Turbo","kW","0.037"]
["","","","M","kW","0.015"]
["","","","L","kW","0.010"]
["","","","Tichý","kW","0.008"]
["Hladina akustického tlaku","Prevádzka čističky vzduchu","","Turbo","dBA","53"]
["","","","Stredný","dBA","39"]
["","","","Nízka","dBA","29"]
["","","","Tichý","dBA","19"]
["Fan","Prietok vzduchu","Prevádzka čističky vzduchu","Turbo","m³/h","330"]
["","","","Stredný","m³/h","192"]
["","","","Nízka","m³/h","120"]
["","","","Tichý","m³/h","66"]
["Metóda zachytávania prachu","","","","","Elektrostatický filter HEPA"]
["Deodorizing method","","","","","Flash Streamer + deodorizačný katalyzátor"]
["Bezpečnostné zariadenia","Položka","","01","","Safety switch (Operation stops when the Streamer unit cover is open)"]
["Štandardné príslušenstvo","Diaľkový ovládač","","","","1"]
["","Držiak diaľkového ovládača","","","","1"]
["","Elektrostatický filter HEPA","","","","1"]
["","Deodorizačný filter","","","","1"]
["","Návod na prevádzku","","","","1"]
["Napájací kábel","m","","","","1.8"]
["Power supply","Phase","","","","1~"]
["","Frekvencia","","","Hz","50/60"]
["","Napätie","","","V","220-240/220-230"]
["Prevádzkový prúd","Prevádzka čističky vzduchu","","Turbo","A","0.32"]
["","","","Stredný","A","0.14"]
["","","","Nízka","A","0.10"]
["","","","Tichý","A","0.08"]
["Poznámky","","","","","(1) - Hodnota pre vhodnú plochu v miestnosti platí pre prevádzku jednotky s maximálnou rýchlosťou ventilátora (HH). Použiteľná oblasť v miestnosti určuje priestor, z ktorého môžete do 30 minút odstrániť určité množstvo prachových čiastočiek. (JEM 1467)"]
["","","","","","(2) - Premenené na štandardy NRCC z testovacích hodnôt podľa JEM1467."]
["","","","","","(3) - Premenené na štandardy CADR z testovacích hodnôt podľa JEM1467."]
["","","","","","(4) - Akustické prevádzkové výkony sú priemerné hodnoty namerané vo vzdialenosti 1 m od prednej, ľavej, pravej a hornej strany jednotky. (rovnajú sa hodnotám v bezodrazovej miestnosti)"]
["","","","","","(5) - Elektrostatický filter HEPA je namontovaný v jednotke."]
["","","","","","(6) - Iná funkcia: Aktívna plazmatická funkcia. Funkcia automatického reštartovania."]