{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Typ","","","","","Zvlhčovacia čistička vzduchu"]
["Použitie","","","","","Parapetný typ"]
["Opláštenie","Farba","","","","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","700"]
["","","","Šírka","mm","270"]
["","","","Hĺbka","mm","270"]
["Hmotnosť","Jednotka","","","kg","9.5"]
["Použiteľná oblasť v miestnosti","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Prevádzka čističky vzduchu","Vstup napájania","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Tichý","kW","0.007"]
["Prevádzka zvlhčovania","Vstup napájania","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Tichý","kW","0.011"]
["","Kapacita nádrže na vodu","","","l","2.7"]
["Hladina akustického tlaku","Prevádzka čističky vzduchu","","Turbo","dBA","53.0"]
["","","","Stredný","dBA","39.0"]
["","","","Nízka","dBA","29.0"]
["","","","Tichý","dBA","19.0"]
["","Prevádzka zvlhčovania","","Turbo","dBA","53.0"]
["","","","Stredný","dBA","39.0"]
["","","","Nízka","dBA","33.0"]
["","","","Tichý","dBA","25.0"]
["Ventilátor","Prietok vzduchu","Prevádzka čističky vzduchu","Turbo","m³/h","330"]
["","","","Stredný","m³/h","192"]
["","","","Nízka","m³/h","120"]
["","","","Tichý","m³/h","54"]
["","","Prevádzka zvlhčovania","Turbo","m³/h","330"]
["","","","Stredný","m³/h","192"]
["","","","Nízka","m³/h","144"]
["","","","Tichý","m³/h","102"]
["Metóda zachytávania prachu","","","","","Elektrostatický filter HEPA"]
["Metóda dezodorácie","","","","","Flash Streamer + deodorizačný katalyzátor"]
["Štandardné príslušenstvo","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Napájací kábel","Napájací kábel","","","","1.8"]
["Napájanie","Fáza","","","","1~"]
["Zdroj napájania","Zdroj napájania-=-Frekvencia","","Frekvencia","","50/60"]
["","Zdroj napájania-=-Napätie","","Napätie","","220-240/220-230"]
["Prevádzkový prúd","Prevádzka čističky vzduchu","Prevádzkový prúd-=-Prevádzka čističky vzduchu-=-Turbo","Turbo","","0.50"]
["","","Prevádzkový prúd-=-Prevádzka čističky vzduchu-=-Stredný","Stredný","","0.19"]
["","","Prevádzkový prúd-=-Prevádzka čističky vzduchu-=-Nízka","Nízka","","0.12"]
["","","Prevádzkový prúd-=-Prevádzka čističky vzduchu-=-Tichý","Tichý","","0.09"]
["","Prevádzka zvlhčovania","Prevádzkový prúd-=-Prevádzka zvlhčovania-=-Turbo","Turbo","","0.50"]
["","","Prevádzkový prúd-=-Prevádzka zvlhčovania-=-Stredný","Stredný","","0.20"]
["","","Prevádzkový prúd-=-Prevádzka zvlhčovania-=-Nízka","Nízka","","0.15"]
["","","Prevádzkový prúd-=-Prevádzka zvlhčovania-=-Tichý","Tichý","","0.13"]
["Poznámky","","","","","(1) - Hodnota pre vhodnú plochu v miestnosti platí pre prevádzku jednotky s maximálnou rýchlosťou ventilátora (HH). Použiteľná oblasť v miestnosti určuje priestor, z ktorého môžete do 30 minút odstrániť určité množstvo prachových čiastočiek. (JEM 1467)"]
["","","","","","(2) - Premenené na štandardy NRCC z testovacích hodnôt podľa JEM1467."]