{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Typ","","","","","Zvlhčovacia čistička vzduchu"]
["Použitie","","","","","Parapetný typ"]
["Opláštenie","Farba","","","","Biela (N9. 0)"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","600 (5)"]
["","","","Šírka","mm","395"]
["","","","Hĺbka","mm","287"]
["Hmotnosť","Jednotka","","","kg","12.5"]
["Použiteľná oblasť v miestnosti","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Prevádzka čističky vzduchu","Vstup napájania","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","L","kW","0.01"]
["","","","Tichý","kW","0.008"]
["Prevádzka zvlhčovania","Vstup napájania","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","L","kW","0.012"]
["","","","Tichý","kW","0.011"]
["","Kapacita nádrže na vodu","","","l","3.6"]
["Hladina akustického tlaku","Prevádzka čističky vzduchu","","Turbo","dBA","54"]
["","","","Stredný","dBA","37"]
["","","","Nízka","dBA","27"]
["","","","Tichý","dBA","18"]
["","Prevádzka zvlhčovania","","Turbo","dBA","54"]
["","","","Stredný","dBA","37"]
["","","","Nízka","dBA","27"]
["","","","Tichý","dBA","23"]
["Ventilátor","Prietok vzduchu","Prevádzka čističky vzduchu","Turbo","m³/h","420"]
["","","","Stredný","m³/h","210"]
["","","","Nízka","m³/h","132"]
["","","","Tichý","m³/h","60"]
["","","Prevádzka zvlhčovania","Turbo","m³/h","420"]
["","","","Stredný","m³/h","210"]
["","","","Nízka","m³/h","132"]
["","","","Tichý","m³/h","102"]
["Metóda zachytávania prachu","","","","","Elektrostatický filter HEPA"]
["Metóda dezodorácie","","","","","Flash Streamer + deodorizačný katalyzátor"]
["Štandardné príslušenstvo","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Napájací kábel","m","","","","2"]
["Napájanie","Fáza","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50/60"]
["","Napätie","","","V","220-240/220-230"]
["Poznámky","","","","","(1) - Hodnota pre vhodnú plochu pokrytia platí pre prevádzku jednotky s maximálnou rýchlosťou ventilátora (HH). Oblasť pokrytia určuje priestor, z ktorého môžete do 30 minút odstrániť určité množstvo prachových čiastočiek."]
["","","","","","(2) - Premenené na štandardy NRCC z testovacích hodnôt podľa JEM1467."]
["","","","","","(3) - Akustické prevádzkové výkony sú priemerné hodnoty namerané vo vzdialenosti 1 m od prednej, ľavej, pravej a hornej strany jednotky. (rovnajú sa hodnotám v bezodrazovej miestnosti)"]