{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":5,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","REMA-A"]
[]
[]
[]
[]
["","","","","REMA5A7Y1B"]
["Chladiaci výkon","Nom., c","","kW","14"]
["Rozsah výkonu","HP","","","5"]
["Maximálny počet pripojiteľných vnútorných jednotiek","","","","64 (3)"]
["Vnútorné spojenie indexu","Min.","","","63"]
["","Max.","","","163"]
["Vonkajšie rozmery","Jednotka","Výška","mm","1685"]
["","","Šírka","mm","930"]
["","","Hĺbka","mm","765"]
["Hmotnosť","Jednotka","","kg","213"]
["Ventilátor","Atmosférický tlak vonkajšieho prostredia","Max.","Pa","78"]
["Kompresor","Typ","","","Hermeticky uzavretý scroll kompresor"]
["Prevádz. rozsah","Chladenie","Min.","°CDB","-5"]
["","","Max.","°CDB","46"]
["Prevádzkový rozsah","Kúrenie","Min.","° CWB","-20"]
["","","Max.","° CWB","16"]
["Úroveň akustického výkonu","Chladenie","Men.","dBA","78.3 (5)"]
["Hladina akustického tlaku","Chladenie","Men.","dBA","56.3 (6)"]
["Chladivo","Typ","","","R-32"]
["","GWP","","","675.0"]
["","Náplň","","tCO2Eq","6.08"]
["","Náplň","","kg","9"]
["Pripojenia potrubia","Kvapalina","Typ","","Mosadzné pripojenie"]
["","","OD","mm","9.52"]
["","Plyn","Typ","","Mosadzné pripojenie"]
["","","OD","mm","19.1"]
["","Plyn HP/LP","OD","mm","15.90"]
["Štandardné príslušenstvo","Connection pipes","","","1"]
["","Installation and operation manual","","","1"]
["Napájanie","Názov","","","Y1"]
["","Fáza","","","3N~"]
["Zdroj napájania","Frekvencia","","Hz","50"]
["","Napätie","","V","380-415"]
["Poznámky","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m; výškový rozdiel: 0m"]
["","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m"]
["","","","","(3) - Skutočný počet jednotiek závisí od indexu pripojenia a obmedzení systému."]
["","","","","(4) - Hladina akustického výkonu predstavuje absolútnu hodnotu, ktorú vytvára zdroj hluku."]
["","","","","(5) - Hladina akustického tlaku predstavuje relatívnu hodnotu závislú od vzdialenosti a akustiky. Podrobnosti si prosím pozrite vo výkresoch hladiny hluku."]
["","","","","(6) - RLA vychádza z nasledovných podmienok: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35°CDB"]
["","","","","(7) - V súlade s normou EN/IEC 61000-3-12 môže byť potrebná konzultácia s operátorom rozvodnej siete, aby sa zaistilo, že bude zariadenie pripojené iba k zdroju s hodnotou Ssc  ≥ minimálna hodnota Ssc"]
["","","","","(8) - MCA sa musí použiť na výber správneho rozmeru vodiča. MCA môže byť považovaný za maximálny prevádzkový prúd."]
["","","","","(9) - MFA sa používa na výber ističa a prerušovača obvodu uzemňovacieho pripojenia (prerušovač uzemnenia)."]