{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":20,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RX-K"]
[]
[]
[]
[]
["","","","","","RX20K2V1B","RX20K5V1B","RX20K5V1B9","RX25K2V1B","RX25K5V1B","RX25K5V1B9","RX35K2V1B","RX35K5V1B","RX35K5V1B9","RX50KV1B","RX50K2V1B","RX60KV1B","RX60K2V1B","RX71KV1B","RX71K2V1B"]
["Ventilátor","Prietok vzduchu","Chladenie","Super nízke","m³/min","","","","","","","","","","51.3"]
["","","Kúrenie","Super nízke","m³/min","","","","","","","","","","51.3"]
["","","","Super nízke","cfm","","","","","","","","","","1812"]
["","","Kúrenie","Super nízke","cfm","","","","","","","","","","1812"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","550","550","550","550","550","550","550","550","550","735","734","735","734","735","734"]
["","","","Šírka","mm","658","658","658","658","658","658","658","658","658","870","870","870","870","870","870"]
["","","","Hĺbka","mm","275","275","275","275","275","275","275","275","275","320","373","320","373","320","373"]
["Hmotnosť","Jednotka","","","kg","28","28","28","28","28","28","28","28","28","44","46.0","49","49.0","49","49.0"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10","","-10"]
["","","","Max.","°CDB","46","46","46","46","46","46","46","46","46","46","","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","","-15"]
["","","","Max.","°CWB","18","18","18","18","18","18","18","18","18","18","","18"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","46","46","46","46","46","46","48","48","48","47","","49","","52"]
["","","","Men.","dBA","","","","","","","","","","","47","","49","","52"]
["","Kúrenie","","Vysoké","dBA","47","47","47","47","47","47","48","48","48","48","","49","","52"]
["","","","Men.","dBA","","","","","","","","","","","48","","49","","52"]
["Chladivo","Typ","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Náplň","","","kg","0.74","0.74","0.74","0.74","0.74","0.74","1.0","1.0","1.0","1.13","1.13","1.45","1.45","1.45","1.45"]
["","Náplň","","","tCO2Eq","1.5","1.5","1.5","1.5","1.5","1.5","2.1","2.1","2.1","2.4","2.36","3.0","3.03","3.0","3.03"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","15","15","15","15","15","15","15","15","15","30","30.0","30","30.0","30","30.0"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","12","12","12","12","12","12","12","12","12","20","20.0","20","20.0","20","20.0"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["Napájanie","Fáza","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - Prevádzkový rozsah v kombinácii s FTX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s FTX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s FTX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s FTX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s FTX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s FTX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s FTX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s FTX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s FTX-J3: min. 10°CDB ~ max. 46°CDB"]
["Štandardné príslušenstvo","Drain cap","","","","","","","","","","","","","9","9","9","9","9","9"]