{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B9"]
[]
[]
[]
[]
["","","","","","RXA42B5V1B9"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","734"]
["","","","Šírka","mm","954"]
["","","","Hĺbka","mm","401"]
["Hmotnosť","Jednotka","","","kg","49"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","48"]
["","Kúrenie","","Men.","dBA","48"]
["Chladivo","Typ","","","","R-32"]
["","Náplň","","","kg","1.1"]
["","Náplň","","","tCO2Eq","0.75"]
["","GWP","","","","675"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","30"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","20"]
["Štandardné príslušenstvo","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["Napájanie","Fáza","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50"]
["","Napätie","","","V","220-240"]
["Poznámky","","","","","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","(2) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","","(3) - Obsahuje fluórované skleníkové plyny"]