{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-A9"]
[]
[]
[]
[]
["","","","","","RXJ20A5V1B9","RXJ25A5V1B9","RXJ35A5V1B9","RXJ42A5V1B9","RXJ50A5V1B9"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","552","552","552","734","734"]
["","","","Šírka","mm","840","840","840","954","954"]
["","","","Hĺbka","mm","350","350","350","408","408"]
["Hmotnosť","Jednotka","","","kg","32","32","32","49","49"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Max.","°CDB","50","50","50","50","50"]
["","Kúrenie","Okolitá teplota","Min.","° CWB","-21","-21","-21","-21","-21"]
["","","","Max.","° CWB","18","18","18","18","18"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","46","46","49","48","48"]
["","Kúrenie","","Men.","dBA","47","47","49","48","49"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32","R-32"]
["","Náplň","","","kg","0.76","0.76","0.76","1.1","1.1"]
["","Náplň","","","tCO2Eq","0.52","0.52","0.52","0.75","0.75"]
["","GWP","","","","675","675","675","675","675"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","20","20","20","30","30"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","15","15","15","20","20"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1","1","1"]
["","Drain cap","","","","","","","3","3"]
["","Drain plug","","","","1","1","1","1","1"]
["Napájanie","Fáza","","","","1~","1~","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","","(3) - Obsahuje fluórované skleníkové plyny","(3) - Obsahuje fluórované skleníkové plyny","(3) - Obsahuje fluórované skleníkové plyny","(3) - Obsahuje fluórované skleníkové plyny","(3) - Obsahuje fluórované skleníkové plyny"]