{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":16,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-M"]
[]
[]
[]
[]
["","","","","","RXJ20M2V1B","RXJ20M3V1B","RXJ20M5V1B","RXJ25M2V1B","RXJ25M3V1B","RXJ25M5V1B","RXJ35M2V1B","RXJ35M3V1B","RXJ35M5V1B","RXJ50MV1B","RXJ50M2V1B"]
["Ventilátor","Prietok vzduchu","Chladenie","Super nízke","m³/min","29.3","","","29.3","","","29.3","","","38.5"]
["","","Kúrenie","Super nízke","m³/min","25.6","","","25.6","","","25.6","","","34.3"]
["","","","Super nízke","cfm","1035","","","1035","","","1035","","","1359"]
["","","Kúrenie","Super nízke","cfm","904","","","904","","","904","","","1211"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","550","550","550","550","550","550","550","550","550","735","735"]
["","","","Šírka","mm","765","765","765","765","765","765","765","765","765","825","825"]
["","","","Hĺbka","mm","285","285","285","285","285","285","285","285","285","300","300"]
["Hmotnosť","Jednotka","","","kg","34","32","32","34","32","32","34","32","32","44","44"]
["Motor ventilátora","Rýchlosť","Chladenie","Super nízke","ot/min","760","","","760","","","760","","","620"]
["","","Kúrenie","Super nízke","ot/min","740","","","740","","","740","","","620"]
["Kompresor","Type","","","","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46","46","46","46","46","46","46","46","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18","18","18","18","18","18","18","18","20"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","46","","","46","","","48","","","48","48"]
["","","","Men.","dBA","","46","46","","46","46","","49","49"]
["","","","Nízka","dBA","","","","","","","","","","","45"]
["","Kúrenie","","Vysoké","dBA","47","","","47","","","48","","","48","48"]
["","","","Men.","dBA","","47","47","","47","47","","49","49"]
["","","","Nízka","dBA","","","","","","","","","","","45"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Náplň","","","kg","0.72","0.76","0.76","0.72","0.76","0.76","0.72","0.76","0.76","1.30","1.3"]
["","Náplň","","","tCO2Eq","0.5","0.52","0.52","0.5","0.52","0.52","0.5","0.52","0.52","0.9","0.88"]
["","GWP","","","","675","675.0","675.0","675","675.0","675.0","675","675.0","675.0","675","675"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","20","20","20","20","20","20","20","20","20","30","30"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","15","15.0","15.0","15","15.0","15.0","15","15.0","15.0","20"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","","1","1","","1","1","","1"]
["","Drain plug","","","","1","1","","1","1","","1","1","","1"]
["Napájanie","Fáza","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50","50","50","50","50","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - 220 V","","","(1) - 220 V","","","(1) - 220 V","","","(1) - 220 V"]
["","","","","","(2) - 230 V","","","(2) - 230 V","","","(2) - 230 V","","","(2) - 230 V"]
["","","","","","(3) - 240 V","","","(3) - 240 V","","","(3) - 240 V","","","(3) - 240 V"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Štandardné príslušenstvo","Refrigerant charge label","","","","","1","","","1","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1","","","1","","","1"]
["","General safety precautions","","","","","1","","","1","","","1"]