{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":9,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXK-A"]
[]
[]
[]
[]
["","","","","","RXK25AV1B","RXK35AV1B","RXK60AV1B","RXK50AV1B"]
["Hladina akustického tlaku","Kúrenie","","Men.","dBA","45","46","51"]
["","Chladenie","","Men.","dBA","45","46","51"]
["Chladivo","Charge","","","TCO2Eq","1.5","2.1","3.0"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Náplň","","","kg","0.74","1.00","1.45"]
["","Typ","","","","R-410A","R-410A","R-410A"]
["Kompresor","Type","","","","Hermetický rotačný","Hermetický rotačný","Hermetický rotačný"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","658","658","855"]
["","","","Hĺbka","mm","289","289","328"]
["","","","Výška","mm","550","550","753"]
["Hmotnosť","Jednotka","","","kg","24","26","44"]
["Power supply","Fáza","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - Všetky jednotky sú otestované a sú v súlade s normou ISO 5151 (bezkanálová jednotka) alebo ISO 13253 (kanálová jednotka)","(1) - Všetky jednotky sú otestované a sú v súlade s normou ISO 5151 (bezkanálová jednotka) alebo ISO 13253 (kanálová jednotka)","(1) - Všetky jednotky sú otestované a sú v súlade s normou ISO 5151 (bezkanálová jednotka) alebo ISO 13253 (kanálová jednotka)"]
["","","","","","(2) - Všetky špecifikácie môže zmeniť výrobca bez predchádzajúceho upozornenia.","(2) - Všetky špecifikácie môže zmeniť výrobca bez predchádzajúceho upozornenia.","(2) - Všetky špecifikácie môže zmeniť výrobca bez predchádzajúceho upozornenia."]
["","","","","","(3) - Obsahuje fluórované skleníkové plyny","(3) - Obsahuje fluórované skleníkové plyny","(3) - Obsahuje fluórované skleníkové plyny"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","","","628"]
["","","","Šírka","mm","","","","855"]
["","","","Hĺbka","mm","","","","328"]
["Hmotnosť","Jednotka","","","kg","","","","37"]
["Kompresor","Typ","","","","","","","Hermetický rotačný"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","","","","-10"]
["","","","Max.","°CDB","","","","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","","","","-15"]
["","","","Max.","°CWB","","","","18"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","","","","51"]
["","Kúrenie","","Men.","dBA","","","","51"]
["Chladivo","Typ","","","","","","","R-410A"]
["","Náplň","","","kg","","","","1.25"]
["","Náplň","","","tCO2Eq","","","","2.6"]
["","GWP","","","","","","","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","","","","30"]
["Napájanie","Fáza","","","","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","","","50"]
["","Napätie","","","V","","","","220-240"]