{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilátor","Prietok vzduchu","Chladenie","Super nízke","m³/min","30.6","30.6"]
["","","Kúrenie","Super nízke","m³/min","27.2","27.2"]
["","","","Super nízke","cfm","1080","1080"]
["","","Kúrenie","Super nízke","cfm","960","960"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","550","550"]
["","","","Šírka","mm","858","858"]
["","","","Hĺbka","mm","330","330"]
["Hmotnosť","Jednotka","","","kg","40","40"]
["Compressor","Type","","","","","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","-25","-25"]
["","","","Max.","°CWB","18","18"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","48","48"]
["","","","Nízka","dBA","44","44"]
["","Kúrenie","","Vysoké","dBA","49","49"]
["","","","Nízka","dBA","45","45"]
["Chladivo","Typ","","","","R-410A","R-410A"]
["","Náplň","","","kg","1","1"]
["","Náplň","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","20","20"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - IU","Max.","m","15","15"]
["Štandardné príslušenstvo","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Napájanie","Fáza","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","220-240","220-240"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor"]