{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":11,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-N9"]
[]
[]
[]
[]
["","","","","","RXP20N5V1B9","RXP25N5V1B9","RXP35N5V1B9","RXP50N5V1B9","RXP60N5V1B9","RXP71N5V1B9"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","556","556","556","734","734","734"]
["","","","Šírka","mm","740","740","740","954","954","954"]
["","","","Hĺbka","mm","343","343","343","401","401","401"]
["Hmotnosť","Jednotka","","","kg","24","24","26","46","50","50"]
["Kompresor","Type","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°CDB","48","48","48","48","48","48"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18","18","18","18"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","46","46","48"]
["","","","Men.","dBA","","","","47","49","52"]
["","Kúrenie","","Vysoké","dBA","47","47","48"]
["","","","Men.","dBA","","","","49","49","52"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Náplň","","","kg","0.55","0.55","0.70","0.9","1.15","1.15"]
["","Náplň","","","tCO2Eq","0.37","0.37","0.48","0.61","0.78","0.78"]
["","GWP","","","","675.0","675.0","675.0","675","675","675"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","20","20","20","30","30","30"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","12","12","12","20","20","20"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["Napájanie","Fáza","","","","1~","1~","1~","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Štandardné príslušenstvo","Drain cap","","","","","","","3","3","3"]
["Poznámky","","","","","","","","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","","","","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","","","","","(3) - Obsahuje fluórované skleníkové plyny","(3) - Obsahuje fluórované skleníkové plyny","(3) - Obsahuje fluórované skleníkové plyny"]