{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","49","","","52"]
["","","","Nízka","dBA","46","","","49"]
["","Chladenie","","Nízka","dBA","46","","","49"]
["","","","Vysoké","dBA","49","","","52"]
["Štandardné príslušenstvo","Vypúšťacia zásuvka","","","","1","","","1"]
["","Návod na montáž","","","","1","","","1"]
["Chladiace médium","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Náplň","","","kg","1.5","","","2.3"]
["","Typ","","","","R-410A","","","R-410A"]
["Pripojenia potrubia","Úroveň hladiny","IU - OU","Max.","m","20","","","20"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","","","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["Kompresor","Type","","","","Hermeticky utesnený kolísavý kompresor","","","Hermeticky utesnený kolísavý kompresor"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","825","","","900"]
["","","","Hĺbka","mm","300","","","320"]
["","","","Výška","mm","735","","","770"]
["Hmotnosť","Jednotka","","","kg","48","","","71"]
["Power supply","Fáza","","","","1~","","","1~"]
["","Frekvencia","","","Hz","50","","","50"]
["","Napätie","","","V","220-240","","","220-240"]
["Poznámky","","","","","(1) - SL: Režim tichej prevádzky ventilátora s nastavením rýchlosti prietoku vzduchu","(1) - 220 V","","(1) - SL: Režim tichej prevádzky ventilátora s nastavením rýchlosti prietoku vzduchu","(1) - 220 V"]
["","","","","","(2) - Obsahuje fluórované skleníkové plyny","(2) - 230 V","","(2) - Obsahuje fluórované skleníkové plyny","(2) - 230 V"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","735","735","","770","770"]
["","","","Šírka","mm","","825","825","","900","900"]
["","","","Hĺbka","mm","","300","300","","320","320"]
["Hmotnosť","Jednotka","","","kg","","48","48","","71","71"]
["Kompresor","Type","","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","","-10","-10","","-10","-10"]
["","","","Max.","°CDB","","46","46","","46","46"]
["","Kúrenie","Okolitá teplota","Min.","° CWB","","-15","-15","","-15","-15"]
["","","","Max.","° CWB","","18","20","","18","20"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","","49","49","","52","52"]
["","","","Nízka","dBA","","46","46","","49","49"]
["","Kúrenie","","Vysoké","dBA","","49","49","","52","52"]
["","","","Nízka","dBA","","46","46","","49","49"]
["Chladivo","Typ","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Náplň","","","kg","","1.5","1.5","","2.3","2.3"]
["","Náplň","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","","30","30","","30","30"]
["","Dodatočná náplň chladiva","","","kg/m","","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","","20","20","","20","20"]
["Štandardné príslušenstvo","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Napájanie","Fáza","","","","","1~","1~","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","50","50","","50","50"]
["","Napätie","","","V","","220-240","220-240","","220-240","220-240"]
["Poznámky","","","","","","(3) - 240 V","","","(3) - 240 V"]
["Štandardné príslušenstvo","Drain socket","","","","","","1","","","1"]
["Sound power level","Chladenie","","","dBA","","","","65"]