{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Ventilátor","Prietok vzduchu","Chladenie","Super nízke","m³/min","46.0"]
["","","Kúrenie","Super nízke","m³/min","46.0"]
["","","","Super nízke","cfm","1624"]
["","","Kúrenie","Super nízke","cfm","1624"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","770"]
["","","","Šírka","mm","900"]
["","","","Hĺbka","mm","320"]
["Hmotnosť","Jednotka","","","kg","71"]
["Motor ventilátora","Rýchlosť","Chladenie","Super nízke","ot./min.","730"]
["","","Kúrenie","Super nízke","ot./min.","730"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["","Kúrenie","Okolitá teplota","Min.","° CWB","-15"]
["","","","Max.","° CWB","18"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","52"]
["","Kúrenie","","Vysoké","dBA","52"]
["Chladivo","Typ","","","","R-410A"]
["","Náplň","","","kg","2.3"]
["","Náplň","","","tCO2Eq","4.8"]
["","GWP","","","","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","30"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","20"]
["Štandardné príslušenstvo","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Napájanie","Fáza","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50"]
["","Napätie","","","V","220-240"]
["Poznámky","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]