{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","","","48"]
["","Chladenie","","Vysoké","dBA","","","48"]
["Štandardné príslušenstvo","Návod na montáž","","","","","","1"]
["","Štítok s náplňou chladiva","","","","","","1"]
["","Viacjazyčné štítky o fluórovaných skleníkových plynoch","","","","","","1"]
["","Vypúšťacia skrutka (len modely s tepelným čerpadlom)","","","","","","1"]
["Chladiace médium","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Náplň","","","kg","","","1.2"]
["","Typ","","","","","","R-410A"]
["Motor ventilátora","Rýchlosť","Chladenie","Super nízke","ot/min","","","780"]
["","","Kúrenie","Super nízke","ot/min","","","740"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Max.","°CDB","","","46"]
["","","","Min.","°CDB","","","-10"]
["","Kúrenie","Okolitá teplota","Max.","°CWB","","","18"]
["","","","Min.","°CWB","","","-15"]
["Pripojenia potrubia","Úroveň hladiny","IU - OU","Max.","m","","","15"]
["","Dodatočná náplň chladiva","","","kg/m","","","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["Kompresor","Typ","","","","","","Hermeticky utesnený kolísavý kompresor"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","","","765"]
["","","","Hĺbka","mm","","","285"]
["","","","Výška","mm","","","550"]
["Hmotnosť","Jednotka","","","kg","","","34"]
["Ventilátor","Prietok vzduchu","Kúrenie","Super nízke","cfm","","","904"]
["","","","Super nízke","m³/min","","","25.6"]
["","","Chladenie","Super nízke","m³/min","","","30.1"]
["","","","Super nízke","cfm","","","1,063"]
["Power supply","Fáza","","","","","","1~"]
["","Frekvencia","","","Hz","","","50"]
["","Napätie","","","V","","","220-240"]
["Poznámky","","","","","","","(1) - SL: Režim tichej prevádzky ventilátora s nastavením rýchlosti prietoku vzduchu"]
["Ventilátor","Prietok vzduchu","Chladenie","Super nízke","m³/min","30.1","30.1"]
["","","Kúrenie","Super nízke","m³/min","25.6","25.6"]
["","","","Super nízke","cfm","1063","1063"]
["","","Kúrenie","Super nízke","cfm","904","904"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","550","550"]
["","","","Šírka","mm","765","765"]
["","","","Hĺbka","mm","285","285"]
["Hmotnosť","Jednotka","","","kg","34","34"]
["Motor ventilátora","Rýchlosť","Chladenie","Super nízke","ot/min","780","780"]
["","","Kúrenie","Super nízke","ot/min","740","740"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","-15","-15"]
["","","","Max.","°CWB","18","18"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","46","46"]
["","Kúrenie","","Vysoké","dBA","47","47"]
["Chladivo","Typ","","","","R-410A","R-410A"]
["","Náplň","","","kg","1.0","1.0"]
["","Náplň","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","20","20"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","15","15"]
["Štandardné príslušenstvo","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Napájanie","Fáza","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","220-240","220-240"]
["Poznámky","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]
["Štandardné príslušenstvo","Drain plug (only heat pump models)","","","","","1"]