{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-A"]
[]
[]
[]
[]
["","","","","","RXTP25A2V1B","RXTP35A2V1B"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","605","605"]
["","","","Šírka","mm","930","930"]
["","","","Hĺbka","mm","376","376"]
["Hmotnosť","Jednotka","","","kg","42","42"]
["Motor ventilátora","Rýchlosť","Chladenie","Super nízke","ot./min.","800","800"]
["","","Kúrenie","Super nízke","ot./min.","400","400"]
["Compressor","Typ","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Kúrenie","Okolitá teplota","Min.","° CWB","-31","-31"]
["","","","Max.","° CWB","18","18"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","48","48"]
["","Kúrenie","","Men.","dBA","49.0","49.0"]
["Chladivo","Typ","","","","R-32","R-32"]
["","Náplň","","","kg","0.97","0.97"]
["","Náplň","","","tCO2Eq","0.66","0.66"]
["","GWP","","","","675.0","675.0"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","20","20"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","15.0","15.0"]
["Štandardné príslušenstvo","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["Napájanie","Fáza","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","220-240","220-240"]