{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N9"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B9","RXTP35N2V1B9"]
["Hladina akustického tlaku","Kúrenie","","Men.","dBA","49","49"]
["","Chladenie","","Men.","dBA","48","48"]
["Štandardné príslušenstvo","Návod na montáž","","","","1","1"]
["","Štítok s náplňou chladiva","","","","1","1"]
["","Viacjazyčné štítky o fluórovaných skleníkových plynoch","","","","1","1"]
["Chladiace médium","Charge","","","TCO2Eq","0.75","0.75"]
["","GWP","","","","675","675"]
["","Náplň","","","kg","1.1","1.1"]
["","Typ","","","","R-32","R-32"]
["Motor ventilátora","Počet otáčok","Chladenie","Super nízke","ot./min.","450","450"]
["","","Vykurovanie","Super nízke","ot./min.","360","360"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Max.","°CDB","46","46"]
["","","","Min.","°CDB","-10","-10"]
["","Kúrenie","Okolitá teplota","Max.","°CWB","18","18"]
["","","","Min.","°CWB","-25","-25"]
["Pripojenia potrubia","Úroveň hladiny","IU - OU","Max.","m","15","15"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["Kompresor","Type","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","763","763"]
["","","","Hĺbka","mm","312","312"]
["","","","Výška","mm","551","551"]
["Hmotnosť","Jednotka","","","kg","38","38"]
["Power supply","Fáza","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Poznámky","","","","","(1) - Obsahuje fluórované skleníkové plyny","(1) - Obsahuje fluórované skleníkové plyny"]
["","","","","","(2) - Prevádzkový rozsah nájdete v samostatnom výkrese","(2) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","(3) - Elektrické údaje nájdete v samostatných nákresoch","(3) - Elektrické údaje nájdete v samostatných nákresoch"]