{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","","","48","48","50","50"]
["","Chladenie","","Vysoké","dBA","","","48","48","49","49"]
["Štandardné príslušenstvo","Návod na prevádzku","","","","","","1","1","1","1"]
["","Návod na montáž","","","","","","1","1","1","1"]
["Chladiace médium","GWP","","","","","","675","675","675","675"]
["","Náplň","","","kg","","","1.34","1.34","1.34","1.34"]
["","Typ","","","","","","R-32","R-32","R-32","R-32"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Max.","°CDB","","","43","43","43","43"]
["","","","Min.","°CDB","","","-10","-10","-10","-10"]
["","Kúrenie","Okolitá teplota","Max.","° CWB","","","18","18","18","18"]
["","","","Min.","° CWB","","","-20","-20","-20","-20"]
["Pripojenia potrubí","Úroveň hladiny","IU - OU","Max.","m","","","8","8","8","8"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","","","795","795","795","795"]
["","","","Hĺbka","mm","","","300","300","300","300"]
["","","","Výška","mm","","","693","693","693","693"]
["Kompresor","Typ","","","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Hmotnosť","Jednotka","","","kg","","","50","50","50","50"]
["Power supply","Fáza","","","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","","","50","50","50","50"]
["","Napätie","","","V","","","220-240","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","","","(4) - Obsahuje fluórované skleníkové plyny","(4) - Obsahuje fluórované skleníkové plyny","(4) - Obsahuje fluórované skleníkové plyny","(4) - Obsahuje fluórované skleníkové plyny"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","693","693"]
["","","","Šírka","mm","795","795"]
["","","","Hĺbka","mm","300","300"]
["Hmotnosť","Jednotka","","","kg","50","50"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","43","43"]
["","Kúrenie","Okolitá teplota","Min.","° CWB","-20","-20"]
["","","","Max.","° CWB","18","18"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","46","46"]
["","Kúrenie","","Vysoké","dBA","46","46"]
["Chladivo","Typ","","","","R-32","R-32"]
["","Náplň","","","kg","1.34","1.34"]
["","Náplň","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","10","10"]
["","Úroveň hladiny","IU - OU","Max.","m","8","8"]
["Štandardné príslušenstvo","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Napájanie","Fáza","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","220-240","220-240"]