{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","870","870"]
["","","","Šírka","mm","1,100","1,100"]
["","","","Hĺbka","mm","460","460"]
["Hmotnosť","Jednotka","","","kg","117","117"]
["Kompresor","Typ","","","","Hermeticky utesnený skrutkový kompresor","Hermeticky utesnený skrutkový kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-20","-20"]
["","","","Max.","°CDB","46","46"]
["","Kúrenie","Okolitá teplota","Min.","° CWB","-20","-20"]
["","","","Max.","° CWB","15","15"]
["Úroveň akustického výkonu","Chladenie","","","dBA","73","76"]
["","Vykurovanie","","","dBA","76 (1)","79 (1)"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","53","57"]
["","Kúrenie","","Men.","dBA","60","63"]
["Chladivo","Typ","","","","R-32","R-32"]
["","Charge","","","kg","5","5"]
["","GWP","","","","675","675"]
["Pripojenia potrubia","Kvapalina","","OD","mm","9.52","9.52"]
["","Plyn","","OD","mm","22.2","22.2"]
["","Dĺžka potrubia","Max.","OU - IU","m","100","100"]
["","","Systém","Bez náplne","m","30","30"]
["","Dodatočná náplň chladiva","","","kg/m","Pozrite si inštalačnú príručku","Pozrite si inštalačnú príručku"]
["Štandardné príslušenstvo","Návod na montáž","","","","1","1"]
["","Všeobecné bezpečnostné opatrenia","","","","1","1"]
["","Upínacie pásy","","","","2","2"]
["","Odlepiteľná nálepka F-plyn","","","","1","1"]
["","Pripájanie potrubia","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","380-415","380-415"]
["Prúd - 50Hz","Maximálne istenie (MFA)","","","A","20","20"]
["Poznámky","","","","","(1) - Podľa ENER Lot 21","(1) - Podľa ENER Lot 21"]