{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","1,680"]
["","","","Šírka","mm","930"]
["","","","Hĺbka","mm","765"]
["Hmotnosť","Jednotka","","","kg","183.0"]
["Kompresor","Typ","","","","Hermeticky utesnený skrutkový kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-5.0"]
["","","","Max.","°CDB","46.0"]
["","Kúrenie","Okolitá teplota","Min.","° CWB","-15.0"]
["","","","Max.","° CWB","15.0"]
["Sound power level","Chladenie","","","dBA","78.0"]
["","Vykurovanie","","","dBA","78.0"]
["Chladiace médium","Typ","","","","R-410A"]
["","Charge","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Pripojenia potrubia","Kvapalina","","OD","mm","9.52"]
["","Plyn","","OD","mm","22.2"]
["","Dĺžka potrubia","Max.","OU - IU","m","100"]
["","","Systém","Bez náplne","m","30"]
["Štandardné príslušenstvo","Návod na montáž","","","","1"]
["","Pripájanie potrubia","","","","4"]
["Power supply","Fáza","","","","3N~"]
["","Frekvencia","","","Hz","50"]
["","Napätie","","","V","380-415"]
["Prúd - 50Hz","Maximálne istenie (MFA)","","","A","25"]
["Poznámky","","","","","(1) - Napájanie vnútornej jednotky FDQ je samostatné"]
["","","","","","(2) - Pozrite si samostatné nákresy s elektrickými údajmi"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","1680"]
["","","","Šírka","mm","","930"]
["","","","Hĺbka","mm","","765"]
["Hmotnosť","Jednotka","","","kg","","184.0"]
["Kompresor","Typ","","","","","Hermeticky uzavretý scroll kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","","-5.0"]
["","","","Max.","°CDB","","46.0"]
["","Kúrenie","Okolitá teplota","Min.","° CWB","","-15.0"]
["","","","Max.","° CWB","","15.0"]
["Akustický výkon","Chladenie","","","dBA","","78.0"]
["","Vykurovanie","","","dBA","","78.0"]
["Chladivo","Náplň","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Náplň","","","tCO2Eq","","19.4"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","12.70"]
["","Plyn","","OD","mm","","22.2"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","","100"]
["","","Systém","Bez náplne","m","","30"]
["Štandardné príslušenstvo","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Zdroj napájania","Frekvencia","","","Hz","","50"]
["Istenie – 50 Hz","Maximálne istenie (MFA)","","","A","","25"]