{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Hladina akustického tlaku","Kúrenie","Vysoké","dBA","38"]
["","","Stredný","dBA","36"]
["","","Nízka","dBA","30"]
["","Chladenie","Stredný","dBA","36"]
["","","Nízka","dBA","30"]
["","","Vysoké","dBA","38"]
["Štandardné príslušenstvo","Návod na montáž","","","1"]
["","Návod na prevádzku","","","1"]
["","Izolácia príslušenstva","","","1"]
["","Tesniaca podložka","","","1"]
["","Kovová svorka","","","1"]
["","Vypúšťacia hadica","","","1"]
["","Podložka pre držiak ramena","","","8"]
["","Tesniaci materiál","","","2"]
["","Svorky","","","6"]
["","Upevňovacia doska podložky","","","4"]
["","Skrutky na príruby potrubia","","","1"]
["","Vzduchový filter","","","1"]
["Pripojenia potrubia","Kvapalina","OD","mm","6.35"]
["","Plyn","OD","mm","12.7"]
["","Vypúšťanie","","","VP20 (I.D. 20/O.D. 26)"]
["Vstup napájania","Chladenie","Men.","kW","0.060"]
["","Kúrenie","Men.","kW","0.060"]
["Sound power level","Chladenie","","dBA","55"]
["","Vykurovanie","","dBA","55"]
["Vonkajšie rozmery","Jednotka","Šírka","mm","1,150"]
["","","Hĺbka","mm","620"]
["","","Výška","mm","200"]
["Hmotnosť","Jednotka","","kg","30.0"]
["Ventilátor","Externý statický tlak","Nom. ot.","Pa","40"]
["Power supply","Fáza","","","1~"]
["","Frekvencia","","Hz","50/60"]
["","Názov","","","VE"]
["","Napätie","","V","220-240"]
["Poznámky","","","","(1) - Pri spojení s viacsystémovou vonkajšou jednotkou si preštudujte technické údaje viacsystémovej vonkajšej jednotky, ktorú chcete pripojiť."]